|  |
| --- |
| Photo displaying partial image of two pie charts on a canvas-textured page |
| فارمنگ مشین  آپریٹر گائیڈ |
| |  |  |  | | --- | --- | --- | | *Prepared By: Engr. Haseeb Ashfaq* |  | **فارورڈ سپورٹس (پرائیویٹ) لیمیٹڈ** | |

**TABLE OF CONTENTS**

1. **MACHINE PARTS**
2. **MACHINE OPERATING PROCEDURE**
3. **SAFETY/PRECATIONS**

**MACHINE PARTS**

1. **ELECTRIC PANEL**
2. **SENSORS**
3. **SOLENOID VALVES**
4. **VACUME BLOWER**
5. **PUSH BUTTONS**
6. **PRESSURE GUAGE**
7. **PRESSURE SWITCHES**

**MACHINE OPERATING PROCEDURE**

|  |  |
| --- | --- |
| **ENGLISH** | **اردو** |
| 1. **SWITCH ON THE MACHINE.** |  |
| 1. **PLACE THE SHEET BELOW THE MACHINE HEAD** |  |
| 1. **PRESS THE OPERATING BUTTON** |  |
| 1. **WAIT FOR THE HEAD TO CUT THE SHEET** |  |
| 1. **AFTER THE HEAD GOES BACK TO ITS ORIGINAL POSITION PICK UP THE SHEET** |  |
| 1. **REPEAT THE SAME CYCLE** |  |
|  |  |
|  |  |

**SAFETY/PRECATIONS**

|  |  |
| --- | --- |
| **ENGLISH** | **اردو** |
| 1. **MACHINE CLEANING MUST BE DONE ON DAILY BASIS** |  |
| 1. **OPERATOR ALWAYS OPERATE THE MACHINE WHILE STANDING ON THE RUBBER MAT** |  |
| 1. **ELECTRIC PANEL WIRING MUST BE PROPER** |  |
| 1. **OPERATOR SHOULD NEVER INSERT HIS/HER HANDS BETWEEN THE HEAD AND THE BED OF THE MACHINE** |  |
| 1. **EMERGENCEY SHOULD BE WORKING** |  |
| 1. **CALL MAINTENANCE TEAM FOR ANY KIND OF ABNORMALITY** |  |